
HANDCUFFS

POLICE SPEEDCUFFS –Semi Fixed

[image: image1.png]



FEATURES

· Affordable top quality handcuff supplied with two standard handcuff keys.

· Double ratchet locking system.

· High tensile spring (56-58 HRC) per each.

· Reinforced steel swivels on chain handcuff.

· Heavy-duty (5mm) solid hinge on link handcuff

· 13 Locking positions on 4mm thick cuff.

· Cuff holder 2,5mm thick per side.

· Material: Hot rolled C.Q. P.O. prime.

· Nickel-plated to a gloss shine and temporal or black chrome for non-reflection.

HEAVY-DUTY LEG IRONS
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· Constructed from Galvanized mild steel. 

· Adjustable, pad lockable padlock.

· Leg cuffs with keys, belly chains and escort chains also available.









